{"text_format":"3","workbook":"xls","n_sheets":3,"sheets":["Sheet1","Sheet2","Sheet3"],"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet1","index":0,"n_rows":52,"n_cols":11,"rows_kept":52,"merged":[[0,0,0,10],[2,0,3,0],[4,0,5,0],[6,0,7,0],[8,0,9,0],[10,0,11,0],[12,0,13,0],[14,0,15,0],[16,0,17,0],[18,0,19,0],[20,0,21,0],[22,0,23,0],[24,0,25,0],[26,0,27,0],[28,0,29,0],[30,0,31,0],[32,0,33,0],[34,0,37,0],[38,0,39,0],[40,0,41,0],[42,0,43,0],[44,0,47,0],[50,1,50,10],[51,0,52,10]],"flags":["formulas_cached_only"]}
["附件一："]
["楼栋号","编号（自左到右）","宽（mm）","深（mm）","提升高度","提升层数\n（例：24+1）","速度\n（m/s）","基坑深度\n（m）","冲顶高度\n（m）","消防电梯\n（是/否）","备注"]
["1#楼","电梯1",2100,2200,80.7,"27+1",1.5,1.6,4.7,"是"]
[null,"电梯2",2100,2200,80.7,"27+1",1.5,1.6,4.7]
["2#楼","电梯1",2100,2200,80.7,"27+1",1.5,1.6,4.7,"是"]
[null,"电梯2",2100,2200,80.7,"27+1",1.5,1.6,4.7]
["3#楼","电梯1",2100,2200,80.7,"27+1",1.5,1.6,4.7,"是"]
[null,"电梯2",2100,2200,80.7,"27+1",1.5,1.6,4.7]
["4#楼","电梯1",2100,2200,80.7,"27+1",1.5,1.6,4.7,"是"]
[null,"电梯2",2100,2200,80.7,"27+1",1.5,1.6,4.7]
["5#楼","电梯1",2100,2200,80.7,"27+1",1.5,1.6,4.7,"是"]
[null,"电梯2",2100,2200,80.7,"27+1",1.5,1.6,4.7]
["6#楼","电梯1",2100,2200,72,"24+1",1.5,1.6,4.7,"是"]
[null,"电梯2",2100,2200,72,"24+1",1.5,1.6,4.7]
["7#楼","电梯1",2100,2350,28.9,"9+1",1.5,1.6,4.7,null,"贯穿式电梯\n"]
[null,"电梯2",2100,2350,28.9,"9+1",1.5,1.6,4.7,null,"贯穿式电梯"]
["8#楼","电梯1",2100,2350,28.9,"9+1",1.5,1.6,4.7,null,"贯穿式电梯"]
[null,"电梯2",2100,2350,28.9,"9+1",1.5,1.6,4.7,null,"贯穿式电梯"]
["9#楼","电梯1",2100,2200,54.6,"18+1",1.5,1.6,4.7,"是"]
[null,"电梯2",2000,2200,54.6,"18+1",1.5,1.6,4.7]
["10#楼","电梯1",2100,2350,28.9,"9+1",1.5,1.6,4.7,null,"贯穿式电梯"]
[null,"电梯2",2100,2350,28.9,"9+1",1.5,1.6,4.7,null,"贯穿式电梯"]
["11#楼","电梯1",2100,2200,80.7,"27+1",1.5,1.6,4.7,"是"]
[null,"电梯2",2100,2200,80.7,"27+1",1.5,1.6,4.7]
["12#楼","电梯1",2100,2200,60.4,"20+1",1.5,1.6,4.7,"是"]
[null,"电梯2",2100,2200,60.4,"20+1",1.5,1.6,4.7]
["13#楼","电梯1",2100,2350,28.9,"9+1",1.5,1.6,4.7,null,"贯穿式电梯"]
[null,"电梯2",2100,2350,28.9,"9+1",1.5,1.6,4.7,null,"贯穿式电梯"]
["14#楼","电梯1",2100,2200,54.6,"18+1",1.5,1.6,4.7,"是"]
[null,"电梯2",2000,2200,54.6,"18+1",1.5,1.6,4.7]
["15#楼","电梯1",2100,2350,28.9,"9+1",1.5,1.6,4.7,null,"贯穿式电梯"]
[null,"电梯2",2100,2350,28.9,"9+1",1.5,1.6,4.7,null,"贯穿式电梯"]
["16#楼","电梯1",2100,2200,66.2,"22+1",1.5,1.6,4.7,"是"]
[null,"电梯2",2100,2200,66.2,"22+1",1.5,1.6,4.7]
["17#楼","电梯1",2100,2200,54.6,"18+1",1.5,1.6,4.7,"是"]
[null,"电梯2",2000,2200,54.6,"18+1",1.5,1.6,4.7]
[null,"电梯3",2000,2200,54.6,"18+1",1.5,1.6,4.7]
[null,"电梯4",2100,2200,54.6,"18+1",1.5,1.6,4.7,"是"]
["18#楼","电梯1",2100,2350,28.9,"9+1",1.5,1.6,4.7,null,"贯穿式电梯"]
[null,"电梯2",2100,2350,28.9,"9+1",1.5,1.6,4.7,null,"贯穿式电梯"]
["19#楼","电梯1",2100,2350,34.8,"11+1",1.5,1.6,4.7,null,"贯穿式电梯"]
[null,"电梯2",2100,2350,34.8,"11+1",1.5,1.6,4.7,null,"贯穿式电梯"]
["20#楼","电梯1",2100,2350,28.9,"9+1",1.5,1.6,4.7,null,"贯穿式电梯"]
[null,"电梯2",2100,2350,28.9,"9+1",1.5,1.6,4.7,null,"贯穿式电梯"]
["21#楼","电梯1",2100,2200,54.6,"18+1",1.5,1.6,4.7,"是"]
[null,"电梯2",2000,2200,54.6,"18+1",1.5,1.6,4.7]
[null,"电梯3",2000,2200,54.6,"18+1",1.5,1.6,4.7]
[null,"电梯4",2100,2200,54.6,"18+1",1.5,1.6,4.7,"是"]
["S5#","电梯",2200,2100,9.3,2,1,1.6,4.7]
["S1#","电梯",2200,2300,8.4,3,1,1.6,5.5,null,"无机房贯穿电梯"]
["合计：","48台"]
["注：1、电梯内安装电动车探测器，并保证电动车进入电梯后，电梯无法提升；\n2、本次电梯使用无线五方通话系统；\n3、无障碍电梯至少设置残疾人面板及扶手；\n4、有机房电梯电梯首层门及负一层门不锈钢材质，其余层数使用喷塑钢板。S5和S1电梯门使用不锈钢材质；\n5、主机需预留满足消防联动的接口等。"]

{"sheet":"Sheet2","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}

{"sheet":"Sheet3","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"flags":["formulas_cached_only"]}